FDC LOG
Reset
FD 0 Off
Drive control (00) <2D ><2D >>
Reset
FD 0 Off
Drive control (00) <2D ><2D >>
Reset
FD 0 Off
Drive control (00) <2D ><2D >>
Reset
FD 0 Off
Drive control (00) <2D ><2D >>

[03] Specify FD 1 On
(da 19)
FD 1 Off

[07] Recalibrate FD 1 On
(00)
Seek: 0 -> 0 (0)
FD 1 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 00 }
FD 1 Off

[07] Recalibrate FD 0 On
(00)
Seek: 0 -> 0 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 00 }
FD 0 Off

[0f] Seek FD 0 On
(00 0a)
Seek: 0 -> 20 (20)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0a }
FD 0 Off

[07] Recalibrate FD 0 On
(00)
Seek: 20 -> 0 (20)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 00 }
FD 0 Off

[07] Recalibrate FD 0 On
(01)
Seek: 0 -> 0 (0)
FD 0 Off
	Seek (1) success.

[08] SenceIntStatus 	{ 21 00 }
FD 0 Off

[07] Recalibrate FD 1 On
(01)
Seek: 0 -> 0 (0)
FD 1 Off
	Seek (1) success.

[08] SenceIntStatus 	{ 21 00 }
FD 1 Off

[0f] Seek FD 1 On
(01 0a)
Seek: 0 -> 20 (20)
FD 1 Off
	Seek (1) success.

[08] SenceIntStatus 	{ 21 0a }
FD 1 Off

[07] Recalibrate FD 1 On
(01)
Seek: 20 -> 0 (20)
FD 1 Off
	Seek (1) success.

[08] SenceIntStatus 	{ 21 00 }
FD 1 Off

[04] SenceDeviceStatus FD 1 On
(00) 	{ 3c }
FD 1 Off
Drive control (00) <2D ><2D >>
Drive control (00) <2D ><2D >>

[03] Specify FD 0 On
(da 19)
FD 0 Off
Drive control (00) <2D ><2D >>

[0f] Seek FD 0 On
(00 00)
Seek: 0 -> 0 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 00 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 3c }
FD 0 Off

[46] ReadData FD 0 On
(00 00 00 01 01 10 0e ff)
	Read 00 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 00 00 02 01 }
FD 0 Off

[07] Recalibrate FD 0 On
(01)
Seek: 0 -> 0 (0)
FD 0 Off
	Seek (1) success.

[08] SenceIntStatus 	{ 21 00 }
FD 0 Off

[07] Recalibrate FD 1 On
(01)
Seek: 0 -> 0 (0)
FD 1 Off
	Seek (1) success.

[08] SenceIntStatus 	{ 21 00 }
FD 1 Off

[0f] Seek FD 1 On
(01 05)
Seek: 0 -> 10 (10)
FD 1 Off
	Seek (1) success.

[08] SenceIntStatus 	{ 21 05 }
FD 1 Off

[07] Recalibrate FD 1 On
(01)
Seek: 10 -> 0 (10)
FD 1 Off
	Seek (1) success.

[08] SenceIntStatus 	{ 21 00 }
FD 1 Off
Drive control (00) <2D ><2D >>
Drive control (00) <2D ><2D >>
Drive control (00) <2D ><2D >>

[0f] Seek FD 1 On
(00 01)
Seek: 0 -> 2 (2)
FD 1 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 01 }
FD 1 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 01 00 01 01 10 0e ff)
	Read 01 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 01 00 02 01 }
FD 0 Off
Drive control (00) <2D ><2D >>

[0f] Seek FD 0 On
(00 01)
Seek: 2 -> 2 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 01 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 01 00 02 01 10 0e ff)
	Read 01 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 01 00 03 01 }
FD 0 Off
Drive control (00) <2D ><2D >>

[0f] Seek FD 0 On
(00 01)
Seek: 2 -> 2 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 01 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 01 00 03 01 10 0e ff)
	Read 01 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 01 00 04 01 }
FD 0 Off
Drive control (00) <2D ><2D >>

[0f] Seek FD 0 On
(00 01)
Seek: 2 -> 2 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 01 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 01 00 04 01 10 0e ff)
	Read 01 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 01 00 05 01 }
FD 0 Off
Drive control (00) <2D ><2D >>

[0f] Seek FD 0 On
(00 01)
Seek: 2 -> 2 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 01 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 01 00 05 01 10 0e ff)
	Read 01 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 01 00 06 01 }
FD 0 Off
Drive control (00) <2D ><2D >>

[0f] Seek FD 0 On
(00 01)
Seek: 2 -> 2 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 01 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 01 00 06 01 10 0e ff)
	Read 01 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 01 00 07 01 }
FD 0 Off
Drive control (00) <2D ><2D >>

[0f] Seek FD 0 On
(00 01)
Seek: 2 -> 2 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 01 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 01 00 07 01 10 0e ff)
	Read 01 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 01 00 08 01 }
FD 0 Off
Drive control (00) <2D ><2D >>

[0f] Seek FD 0 On
(00 02)
Seek: 2 -> 4 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 08 01 10 0e ff)
	Read 02 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 27)
Seek: 4 -> 78 (74)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 27 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 27 01 01 01 10 0e ff)
	Read 27 01 01 01

	Read 27 01 02 01

	Read 27 01 03 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 27 01 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 78 -> 4 (74)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 06)
Seek: 4 -> 12 (8)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 06 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 06 00 01 01 10 0e ff)
	Read 06 00 01 01

	Read 06 00 02 01

	Read 06 00 03 01

	Read 06 00 04 01

	Read 06 00 05 01

	Read 06 00 06 01

	Read 06 00 07 01

	Read 06 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 06 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 06)
Seek: 12 -> 12 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 06 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 06 00 09 01 10 0e ff)
	Read 06 00 09 01

	Read 06 00 0a 01

	Read 06 00 0b 01

	Read 06 00 0c 01

	Read 06 00 0d 01

	Read 06 00 0e 01

	Read 06 00 0f 01

	Read 06 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 07 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 06)
Seek: 12 -> 12 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 06 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 06 01 01 01 10 0e ff)
	Read 06 01 01 01

	Read 06 01 02 01

	Read 06 01 03 01

	Read 06 01 04 01

	Read 06 01 05 01

	Read 06 01 06 01

	Read 06 01 07 01

	Read 06 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 06 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 06)
Seek: 12 -> 12 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 06 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 06 01 09 01 10 0e ff)
	Read 06 01 09 01

	Read 06 01 0a 01

	Read 06 01 0b 01

	Read 06 01 0c 01

	Read 06 01 0d 01

	Read 06 01 0e 01

	Read 06 01 0f 01

	Read 06 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 07 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 07)
Seek: 12 -> 14 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 07 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 07 00 01 01 10 0e ff)
	Read 07 00 01 01

	Read 07 00 02 01

	Read 07 00 03 01

	Read 07 00 04 01

	Read 07 00 05 01

	Read 07 00 06 01

	Read 07 00 07 01

	Read 07 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 07 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 07)
Seek: 14 -> 14 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 07 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 07 00 09 01 10 0e ff)
	Read 07 00 09 01

	Read 07 00 0a 01

	Read 07 00 0b 01

	Read 07 00 0c 01

	Read 07 00 0d 01

	Read 07 00 0e 01

	Read 07 00 0f 01

	Read 07 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 08 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 07)
Seek: 14 -> 14 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 07 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 07 01 01 01 10 0e ff)
	Read 07 01 01 01

	Read 07 01 02 01

	Read 07 01 03 01

	Read 07 01 04 01

	Read 07 01 05 01

	Read 07 01 06 01

	Read 07 01 07 01

	Read 07 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 07 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 07)
Seek: 14 -> 14 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 07 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 07 01 09 01 10 0e ff)
	Read 07 01 09 01

	Read 07 01 0a 01

	Read 07 01 0b 01

	Read 07 01 0c 01

	Read 07 01 0d 01

	Read 07 01 0e 01

	Read 07 01 0f 01

	Read 07 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 08 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 08)
Seek: 14 -> 16 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 08 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 08 00 01 01 10 0e ff)
	Read 08 00 01 01

	Read 08 00 02 01

	Read 08 00 03 01

	Read 08 00 04 01

	Read 08 00 05 01

	Read 08 00 06 01

	Read 08 00 07 01

	Read 08 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 08 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 08)
Seek: 16 -> 16 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 08 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 08 00 09 01 10 0e ff)
	Read 08 00 09 01

	Read 08 00 0a 01

	Read 08 00 0b 01

	Read 08 00 0c 01

	Read 08 00 0d 01

	Read 08 00 0e 01

	Read 08 00 0f 01

	Read 08 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 09 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 08)
Seek: 16 -> 16 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 08 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 08 01 01 01 10 0e ff)
	Read 08 01 01 01

	Read 08 01 02 01

	Read 08 01 03 01

	Read 08 01 04 01

	Read 08 01 05 01

	Read 08 01 06 01

	Read 08 01 07 01

	Read 08 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 08 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 08)
Seek: 16 -> 16 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 08 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 08 01 09 01 10 0e ff)
	Read 08 01 09 01

	Read 08 01 0a 01

	Read 08 01 0b 01

	Read 08 01 0c 01

	Read 08 01 0d 01

	Read 08 01 0e 01

	Read 08 01 0f 01

	Read 08 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 09 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 09)
Seek: 16 -> 18 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 09 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 09 00 01 01 10 0e ff)
	Read 09 00 01 01

	Read 09 00 02 01

	Read 09 00 03 01

	Read 09 00 04 01

	Read 09 00 05 01

	Read 09 00 06 01

	Read 09 00 07 01

	Read 09 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 09 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 09)
Seek: 18 -> 18 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 09 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 09 00 09 01 10 0e ff)
	Read 09 00 09 01

	Read 09 00 0a 01

	Read 09 00 0b 01

	Read 09 00 0c 01

	Read 09 00 0d 01

	Read 09 00 0e 01

	Read 09 00 0f 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 09 00 10 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 18 -> 4 (14)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 4 -> 36 (32)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 12 00 01 01 10 0e ff)
	Read 12 00 01 01

	Read 12 00 02 01

	Read 12 00 03 01

	Read 12 00 04 01

	Read 12 00 05 01

	Read 12 00 06 01

	Read 12 00 07 01

	Read 12 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 12 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 36 -> 36 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 12 00 09 01 10 0e ff)
	Read 12 00 09 01

	Read 12 00 0a 01

	Read 12 00 0b 01

	Read 12 00 0c 01

	Read 12 00 0d 01

	Read 12 00 0e 01

	Read 12 00 0f 01

	Read 12 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 13 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 36 -> 36 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 12 01 01 01 10 0e ff)
	Read 12 01 01 01

	Read 12 01 02 01

	Read 12 01 03 01

	Read 12 01 04 01

	Read 12 01 05 01

	Read 12 01 06 01

	Read 12 01 07 01

	Read 12 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 12 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 36 -> 36 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 12 01 09 01 10 0e ff)
	Read 12 01 09 01

	Read 12 01 0a 01

	Read 12 01 0b 01

	Read 12 01 0c 01

	Read 12 01 0d 01

	Read 12 01 0e 01

	Read 12 01 0f 01

	Read 12 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 13 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 36 -> 38 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 13 00 01 01 10 0e ff)
	Read 13 00 01 01

	Read 13 00 02 01

	Read 13 00 03 01

	Read 13 00 04 01

	Read 13 00 05 01

	Read 13 00 06 01

	Read 13 00 07 01

	Read 13 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 13 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 38 -> 38 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 13 00 09 01 10 0e ff)
	Read 13 00 09 01

	Read 13 00 0a 01

	Read 13 00 0b 01

	Read 13 00 0c 01

	Read 13 00 0d 01

	Read 13 00 0e 01

	Read 13 00 0f 01

	Read 13 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 14 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 38 -> 38 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 13 01 01 01 10 0e ff)
	Read 13 01 01 01

	Read 13 01 02 01

	Read 13 01 03 01

	Read 13 01 04 01

	Read 13 01 05 01

	Read 13 01 06 01

	Read 13 01 07 01

	Read 13 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 13 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 38 -> 38 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 13 01 09 01 10 0e ff)
	Read 13 01 09 01

	Read 13 01 0a 01

	Read 13 01 0b 01

	Read 13 01 0c 01

	Read 13 01 0d 01

	Read 13 01 0e 01

	Read 13 01 0f 01

	Read 13 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 14 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 14)
Seek: 38 -> 40 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 14 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 14 00 01 01 10 0e ff)
	Read 14 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 14 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 40 -> 4 (36)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 08 01 10 0e ff)
	Read 02 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 4 -> 74 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 01 01 10 0e ff)
	Read 25 01 01 01

	Read 25 01 02 01

	Read 25 01 03 01

	Read 25 01 04 01

	Read 25 01 05 01

	Read 25 01 06 01

	Read 25 01 07 01

	Read 25 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 25 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 74 -> 74 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 09 01 10 0e ff)
	Read 25 01 09 01

	Read 25 01 0a 01

	Read 25 01 0b 01

	Read 25 01 0c 01

	Read 25 01 0d 01

	Read 25 01 0e 01

	Read 25 01 0f 01

	Read 25 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 26 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 26)
Seek: 74 -> 76 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 26 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 26 00 01 01 10 0e ff)
	Read 26 00 01 01

	Read 26 00 02 01

	Read 26 00 03 01

	Read 26 00 04 01

	Read 26 00 05 01

	Read 26 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 26 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 76 -> 4 (72)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0e)
Seek: 4 -> 28 (24)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0e }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0e 01 09 01 10 0e ff)
	Read 0e 01 09 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0e 01 0a 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 28 -> 4 (24)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 19)
Seek: 4 -> 50 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 19 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 19 01 01 01 10 0e ff)
	Read 19 01 01 01

	Read 19 01 02 01

	Read 19 01 03 01

	Read 19 01 04 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 19 01 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 50 -> 4 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 24)
Seek: 4 -> 72 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 24 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 24 01 01 01 10 0e ff)
	Read 24 01 01 01

	Read 24 01 02 01

	Read 24 01 03 01

	Read 24 01 04 01

	Read 24 01 05 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 24 01 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 72 -> 4 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 4 -> 32 (28)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 10 01 01 01 10 0e ff)
	Read 10 01 01 01

	Read 10 01 02 01

	Read 10 01 03 01

	Read 10 01 04 01

	Read 10 01 05 01

	Read 10 01 06 01

	Read 10 01 07 01

	Read 10 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 10 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 32 -> 32 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 10 01 09 01 10 0e ff)
	Read 10 01 09 01

	Read 10 01 0a 01

	Read 10 01 0b 01

	Read 10 01 0c 01

	Read 10 01 0d 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 10 01 0e 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 32 -> 4 (28)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 4 -> 22 (18)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0b 00 09 01 10 0e ff)
	Read 0b 00 09 01

	Read 0b 00 0a 01

	Read 0b 00 0b 01

	Read 0b 00 0c 01

	Read 0b 00 0d 01

	Read 0b 00 0e 01

	Read 0b 00 0f 01

	Read 0b 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 01 01 10 0e ff)
	Read 0b 01 01 01

	Read 0b 01 02 01

	Read 0b 01 03 01

	Read 0b 01 04 01

	Read 0b 01 05 01

	Read 0b 01 06 01

	Read 0b 01 07 01

	Read 0b 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0b 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 09 01 10 0e ff)
	Read 0b 01 09 01

	Read 0b 01 0a 01

	Read 0b 01 0b 01

	Read 0b 01 0c 01

	Read 0b 01 0d 01

	Read 0b 01 0e 01

	Read 0b 01 0f 01

	Read 0b 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 22 -> 24 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 01 01 10 0e ff)
	Read 0c 00 01 01

	Read 0c 00 02 01

	Read 0c 00 03 01

	Read 0c 00 04 01

	Read 0c 00 05 01

	Read 0c 00 06 01

	Read 0c 00 07 01

	Read 0c 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 09 01 10 0e ff)
	Read 0c 00 09 01

	Read 0c 00 0a 01

	Read 0c 00 0b 01

	Read 0c 00 0c 01

	Read 0c 00 0d 01

	Read 0c 00 0e 01

	Read 0c 00 0f 01

	Read 0c 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0d 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0c 01 01 01 10 0e ff)
	Read 0c 01 01 01

	Read 0c 01 02 01

	Read 0c 01 03 01

	Read 0c 01 04 01

	Read 0c 01 05 01

	Read 0c 01 06 01

	Read 0c 01 07 01

	Read 0c 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 24 -> 4 (20)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 24)
Seek: 4 -> 72 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 24 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 24 00 09 01 10 0e ff)
	Read 24 00 09 01

	Read 24 00 0a 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 24 00 0b 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 72 -> 4 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 4 -> 36 (32)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 12 00 01 01 10 0e ff)
	Read 12 00 01 01

	Read 12 00 02 01

	Read 12 00 03 01

	Read 12 00 04 01

	Read 12 00 05 01

	Read 12 00 06 01

	Read 12 00 07 01

	Read 12 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 12 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 36 -> 36 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 12 00 09 01 10 0e ff)
	Read 12 00 09 01

	Read 12 00 0a 01

	Read 12 00 0b 01

	Read 12 00 0c 01

	Read 12 00 0d 01

	Read 12 00 0e 01

	Read 12 00 0f 01

	Read 12 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 13 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 36 -> 36 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 12 01 01 01 10 0e ff)
	Read 12 01 01 01

	Read 12 01 02 01

	Read 12 01 03 01

	Read 12 01 04 01

	Read 12 01 05 01

	Read 12 01 06 01

	Read 12 01 07 01

	Read 12 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 12 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 36 -> 36 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 12 01 09 01 10 0e ff)
	Read 12 01 09 01

	Read 12 01 0a 01

	Read 12 01 0b 01

	Read 12 01 0c 01

	Read 12 01 0d 01

	Read 12 01 0e 01

	Read 12 01 0f 01

	Read 12 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 13 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 36 -> 38 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 13 00 01 01 10 0e ff)
	Read 13 00 01 01

	Read 13 00 02 01

	Read 13 00 03 01

	Read 13 00 04 01

	Read 13 00 05 01

	Read 13 00 06 01

	Read 13 00 07 01

	Read 13 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 13 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 38 -> 38 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 13 00 09 01 10 0e ff)
	Read 13 00 09 01

	Read 13 00 0a 01

	Read 13 00 0b 01

	Read 13 00 0c 01

	Read 13 00 0d 01

	Read 13 00 0e 01

	Read 13 00 0f 01

	Read 13 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 14 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 38 -> 38 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 13 01 01 01 10 0e ff)
	Read 13 01 01 01

	Read 13 01 02 01

	Read 13 01 03 01

	Read 13 01 04 01

	Read 13 01 05 01

	Read 13 01 06 01

	Read 13 01 07 01

	Read 13 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 13 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 38 -> 38 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 13 01 09 01 10 0e ff)
	Read 13 01 09 01

	Read 13 01 0a 01

	Read 13 01 0b 01

	Read 13 01 0c 01

	Read 13 01 0d 01

	Read 13 01 0e 01

	Read 13 01 0f 01

	Read 13 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 14 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 14)
Seek: 38 -> 40 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 14 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 14 00 01 01 10 0e ff)
	Read 14 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 14 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 40 -> 4 (36)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 08 01 10 0e ff)
	Read 02 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 4 -> 74 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 01 01 10 0e ff)
	Read 25 01 01 01

	Read 25 01 02 01

	Read 25 01 03 01

	Read 25 01 04 01

	Read 25 01 05 01

	Read 25 01 06 01

	Read 25 01 07 01

	Read 25 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 25 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 74 -> 74 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 09 01 10 0e ff)
	Read 25 01 09 01

	Read 25 01 0a 01

	Read 25 01 0b 01

	Read 25 01 0c 01

	Read 25 01 0d 01

	Read 25 01 0e 01

	Read 25 01 0f 01

	Read 25 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 26 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 26)
Seek: 74 -> 76 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 26 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 26 00 01 01 10 0e ff)
	Read 26 00 01 01

	Read 26 00 02 01

	Read 26 00 03 01

	Read 26 00 04 01

	Read 26 00 05 01

	Read 26 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 26 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 76 -> 4 (72)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0e)
Seek: 4 -> 28 (24)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0e }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0e 01 09 01 10 0e ff)
	Read 0e 01 09 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0e 01 0a 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 28 -> 4 (24)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 19)
Seek: 4 -> 50 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 19 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 19 01 01 01 10 0e ff)
	Read 19 01 01 01

	Read 19 01 02 01

	Read 19 01 03 01

	Read 19 01 04 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 19 01 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 50 -> 4 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 24)
Seek: 4 -> 72 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 24 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 24 01 01 01 10 0e ff)
	Read 24 01 01 01

	Read 24 01 02 01

	Read 24 01 03 01

	Read 24 01 04 01

	Read 24 01 05 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 24 01 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 72 -> 4 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 4 -> 32 (28)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 10 01 01 01 10 0e ff)
	Read 10 01 01 01

	Read 10 01 02 01

	Read 10 01 03 01

	Read 10 01 04 01

	Read 10 01 05 01

	Read 10 01 06 01

	Read 10 01 07 01

	Read 10 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 10 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 32 -> 32 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 10 01 09 01 10 0e ff)
	Read 10 01 09 01

	Read 10 01 0a 01

	Read 10 01 0b 01

	Read 10 01 0c 01

	Read 10 01 0d 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 10 01 0e 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 32 -> 4 (28)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 4 -> 22 (18)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0b 00 09 01 10 0e ff)
	Read 0b 00 09 01

	Read 0b 00 0a 01

	Read 0b 00 0b 01

	Read 0b 00 0c 01

	Read 0b 00 0d 01

	Read 0b 00 0e 01

	Read 0b 00 0f 01

	Read 0b 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 01 01 10 0e ff)
	Read 0b 01 01 01

	Read 0b 01 02 01

	Read 0b 01 03 01

	Read 0b 01 04 01

	Read 0b 01 05 01

	Read 0b 01 06 01

	Read 0b 01 07 01

	Read 0b 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0b 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 09 01 10 0e ff)
	Read 0b 01 09 01

	Read 0b 01 0a 01

	Read 0b 01 0b 01

	Read 0b 01 0c 01

	Read 0b 01 0d 01

	Read 0b 01 0e 01

	Read 0b 01 0f 01

	Read 0b 01 10 01

	{ 44 80 00 0c 01 01 01 }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 09 01 10 0e ff)
	Read 0b 01 09 01

	Read 0b 01 0a 01

	Read 0b 01 0b 01

	Read 0b 01 0c 01

	Read 0b 01 0d 01

	Read 0b 01 0e 01

	Read 0b 01 0f 01

	Read 0b 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 22 -> 24 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 01 01 10 0e ff)
	Read 0c 00 01 01

	Read 0c 00 02 01

	Read 0c 00 03 01

	Read 0c 00 04 01

	Read 0c 00 05 01

	Read 0c 00 06 01

	Read 0c 00 07 01

	Read 0c 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 09 01 10 0e ff)
	Read 0c 00 09 01

	Read 0c 00 0a 01

	Read 0c 00 0b 01

	Read 0c 00 0c 01

	Read 0c 00 0d 01

	Read 0c 00 0e 01

	Read 0c 00 0f 01

	Read 0c 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0d 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0c 01 01 01 10 0e ff)
	Read 0c 01 01 01

	Read 0c 01 02 01

	Read 0c 01 03 01

	Read 0c 01 04 01

	Read 0c 01 05 01

	Read 0c 01 06 01

	Read 0c 01 07 01

	Read 0c 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 24 -> 4 (20)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 24)
Seek: 4 -> 72 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 24 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 24 00 09 01 10 0e ff)
	Read 24 00 09 01

	Read 24 00 0a 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 24 00 0b 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 72 -> 4 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 08 01 10 0e ff)
	Read 02 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 4 -> 74 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 01 01 10 0e ff)
	Read 25 01 01 01

	Read 25 01 02 01

	Read 25 01 03 01

	Read 25 01 04 01

	Read 25 01 05 01

	Read 25 01 06 01

	Read 25 01 07 01

	Read 25 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 25 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 74 -> 74 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 09 01 10 0e ff)
	Read 25 01 09 01

	Read 25 01 0a 01

	Read 25 01 0b 01

	Read 25 01 0c 01

	Read 25 01 0d 01

	Read 25 01 0e 01

	Read 25 01 0f 01

	Read 25 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 26 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 26)
Seek: 74 -> 76 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 26 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 26 00 01 01 10 0e ff)
	Read 26 00 01 01

	Read 26 00 02 01

	Read 26 00 03 01

	Read 26 00 04 01

	Read 26 00 05 01

	Read 26 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 26 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 76 -> 4 (72)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0e)
Seek: 4 -> 28 (24)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0e }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0e 01 09 01 10 0e ff)
	Read 0e 01 09 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0e 01 0a 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 28 -> 4 (24)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 19)
Seek: 4 -> 50 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 19 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 19 01 01 01 10 0e ff)
	Read 19 01 01 01

	Read 19 01 02 01

	Read 19 01 03 01

	Read 19 01 04 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 19 01 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 50 -> 4 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 24)
Seek: 4 -> 72 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 24 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 24 01 01 01 10 0e ff)
	Read 24 01 01 01

	Read 24 01 02 01

	Read 24 01 03 01

	Read 24 01 04 01

	Read 24 01 05 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 24 01 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 72 -> 4 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 4 -> 32 (28)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 10 01 01 01 10 0e ff)
	Read 10 01 01 01

	Read 10 01 02 01

	Read 10 01 03 01

	Read 10 01 04 01

	Read 10 01 05 01

	Read 10 01 06 01

	Read 10 01 07 01

	Read 10 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 10 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 32 -> 32 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 10 01 09 01 10 0e ff)
	Read 10 01 09 01

	Read 10 01 0a 01

	Read 10 01 0b 01

	Read 10 01 0c 01

	Read 10 01 0d 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 10 01 0e 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 32 -> 4 (28)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 4 -> 22 (18)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0b 00 09 01 10 0e ff)
	Read 0b 00 09 01

	Read 0b 00 0a 01

	Read 0b 00 0b 01

	Read 0b 00 0c 01

	Read 0b 00 0d 01

	Read 0b 00 0e 01

	Read 0b 00 0f 01

	Read 0b 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 01 01 10 0e ff)
	Read 0b 01 01 01

	Read 0b 01 02 01

	Read 0b 01 03 01

	Read 0b 01 04 01

	Read 0b 01 05 01

	Read 0b 01 06 01

	Read 0b 01 07 01

	Read 0b 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0b 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 09 01 10 0e ff)
	Read 0b 01 09 01

	Read 0b 01 0a 01

	Read 0b 01 0b 01

	Read 0b 01 0c 01

	Read 0b 01 0d 01

	Read 0b 01 0e 01

	Read 0b 01 0f 01

	Read 0b 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 22 -> 24 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 01 01 10 0e ff)
	Read 0c 00 01 01

	Read 0c 00 02 01

	Read 0c 00 03 01

	Read 0c 00 04 01

	Read 0c 00 05 01

	Read 0c 00 06 01

	Read 0c 00 07 01

	Read 0c 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 09 01 10 0e ff)
	Read 0c 00 09 01

	Read 0c 00 0a 01

	Read 0c 00 0b 01

	Read 0c 00 0c 01

	Read 0c 00 0d 01

	Read 0c 00 0e 01

	Read 0c 00 0f 01

	Read 0c 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0d 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0c 01 01 01 10 0e ff)
	Read 0c 01 01 01

	Read 0c 01 02 01

	Read 0c 01 03 01

	Read 0c 01 04 01

	Read 0c 01 05 01

	Read 0c 01 06 01

	Read 0c 01 07 01

	Read 0c 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 24 -> 4 (20)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 08 01 10 0e ff)
	Read 02 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 4 -> 74 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 01 01 10 0e ff)
	Read 25 01 01 01

	Read 25 01 02 01

	Read 25 01 03 01

	Read 25 01 04 01

	Read 25 01 05 01

	Read 25 01 06 01

	Read 25 01 07 01

	Read 25 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 25 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 74 -> 74 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 09 01 10 0e ff)
	Read 25 01 09 01

	Read 25 01 0a 01

	Read 25 01 0b 01

	Read 25 01 0c 01

	Read 25 01 0d 01

	Read 25 01 0e 01

	Read 25 01 0f 01

	Read 25 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 26 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 26)
Seek: 74 -> 76 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 26 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 26 00 01 01 10 0e ff)
	Read 26 00 01 01

	Read 26 00 02 01

	Read 26 00 03 01

	Read 26 00 04 01

	Read 26 00 05 01

	Read 26 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 26 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 76 -> 4 (72)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 18)
Seek: 4 -> 48 (44)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 18 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 18 01 09 01 10 0e ff)
	Read 18 01 09 01

	Read 18 01 0a 01

	Read 18 01 0b 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 18 01 0c 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 48 -> 4 (44)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 19)
Seek: 4 -> 50 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 19 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 19 01 01 01 10 0e ff)
	Read 19 01 01 01

	Read 19 01 02 01

	Read 19 01 03 01

	Read 19 01 04 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 19 01 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 50 -> 4 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 21)
Seek: 4 -> 66 (62)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 21 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 21 00 01 01 10 0e ff)
	Read 21 00 01 01

	Read 21 00 02 01

	Read 21 00 03 01

	Read 21 00 04 01

	Read 21 00 05 01

	Read 21 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 21 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 66 -> 4 (62)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 09 01 10 0e ff)
	Read 0f 01 09 01

	Read 0f 01 0a 01

	Read 0f 01 0b 01

	Read 0f 01 0c 01

	Read 0f 01 0d 01

	Read 0f 01 0e 01

	Read 0f 01 0f 01

	Read 0f 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 10 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 30 -> 32 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 10 00 01 01 10 0e ff)
	Read 10 00 01 01

	Read 10 00 02 01

	Read 10 00 03 01

	Read 10 00 04 01

	Read 10 00 05 01

	Read 10 00 06 01

	Read 10 00 07 01

	Read 10 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 10 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 32 -> 32 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 10 00 09 01 10 0e ff)
	Read 10 00 09 01

	Read 10 00 0a 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 10 00 0b 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 32 -> 4 (28)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 4 -> 22 (18)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0b 00 09 01 10 0e ff)
	Read 0b 00 09 01

	Read 0b 00 0a 01

	Read 0b 00 0b 01

	Read 0b 00 0c 01

	Read 0b 00 0d 01

	Read 0b 00 0e 01

	Read 0b 00 0f 01

	Read 0b 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 01 01 10 0e ff)
	Read 0b 01 01 01

	Read 0b 01 02 01

	Read 0b 01 03 01

	Read 0b 01 04 01

	Read 0b 01 05 01

	Read 0b 01 06 01

	Read 0b 01 07 01

	Read 0b 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0b 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 09 01 10 0e ff)
	Read 0b 01 09 01

	Read 0b 01 0a 01

	Read 0b 01 0b 01

	Read 0b 01 0c 01

	Read 0b 01 0d 01

	Read 0b 01 0e 01

	Read 0b 01 0f 01

	Read 0b 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 22 -> 24 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 01 01 10 0e ff)
	Read 0c 00 01 01

	Read 0c 00 02 01

	Read 0c 00 03 01

	Read 0c 00 04 01

	Read 0c 00 05 01

	Read 0c 00 06 01

	Read 0c 00 07 01

	Read 0c 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 09 01 10 0e ff)
	Read 0c 00 09 01

	Read 0c 00 0a 01

	Read 0c 00 0b 01

	Read 0c 00 0c 01

	Read 0c 00 0d 01

	Read 0c 00 0e 01

	Read 0c 00 0f 01

	Read 0c 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0d 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0c 01 01 01 10 0e ff)
	Read 0c 01 01 01

	Read 0c 01 02 01

	Read 0c 01 03 01

	Read 0c 01 04 01

	Read 0c 01 05 01

	Read 0c 01 06 01

	Read 0c 01 07 01

	Read 0c 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 24 -> 4 (20)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 20)
Seek: 4 -> 64 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 20 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 20 00 09 01 10 0e ff)
	Read 20 00 09 01

	Read 20 00 0a 01

	Read 20 00 0b 01

	Read 20 00 0c 01

	Read 20 00 0d 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 20 00 0e 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 64 -> 4 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 02 01 01 01 10 0e ff)
	Read 02 01 01 01

	Read 02 01 02 01

	Read 02 01 03 01

	Read 02 01 04 01

	Read 02 01 05 01

	Read 02 01 06 01

	Read 02 01 07 01

	Read 02 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 02 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 02 01 09 01 10 0e ff)
	Read 02 01 09 01

	Read 02 01 0a 01

	Read 02 01 0b 01

	Read 02 01 0c 01

	Read 02 01 0d 01

	Read 02 01 0e 01

	Read 02 01 0f 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 02 01 10 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 21)
Seek: 4 -> 66 (62)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 21 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 21 00 01 01 10 0e ff)
	Read 21 00 01 01

	Read 21 00 02 01

	Read 21 00 03 01

	Read 21 00 04 01

	Read 21 00 05 01

	Read 21 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 21 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 66 -> 4 (62)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 09 01 10 0e ff)
	Read 0f 01 09 01

	Read 0f 01 0a 01

	Read 0f 01 0b 01

	Read 0f 01 0c 01

	Read 0f 01 0d 01

	Read 0f 01 0e 01

	Read 0f 01 0f 01

	Read 0f 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 10 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 30 -> 32 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 10 00 01 01 10 0e ff)
	Read 10 00 01 01

	Read 10 00 02 01

	Read 10 00 03 01

	Read 10 00 04 01

	Read 10 00 05 01

	Read 10 00 06 01

	Read 10 00 07 01

	Read 10 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 10 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 32 -> 32 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 10 00 09 01 10 0e ff)
	Read 10 00 09 01

	Read 10 00 0a 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 10 00 0b 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 32 -> 4 (28)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 20)
Seek: 4 -> 64 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 20 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 20 00 09 01 10 0e ff)
	Read 20 00 09 01

	Read 20 00 0a 01

	Read 20 00 0b 01

	Read 20 00 0c 01

	Read 20 00 0d 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 20 00 0e 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 64 -> 4 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 02 01 01 01 10 0e ff)
	Read 02 01 01 01

	Read 02 01 02 01

	Read 02 01 03 01

	Read 02 01 04 01

	Read 02 01 05 01

	Read 02 01 06 01

	Read 02 01 07 01

	Read 02 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 02 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 02 01 09 01 10 0e ff)
	Read 02 01 09 01

	Read 02 01 0a 01

	Read 02 01 0b 01

	Read 02 01 0c 01

	Read 02 01 0d 01

	Read 02 01 0e 01

	Read 02 01 0f 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 02 01 10 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 4 -> 74 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 25 00 01 01 10 0e ff)
	Read 25 00 01 01

	Read 25 00 02 01

	Read 25 00 03 01

	Read 25 00 04 01

	Read 25 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 25 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 74 -> 4 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 03)
Seek: 4 -> 6 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 03 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 03 01 01 01 10 0e ff)
	Read 03 01 01 01

	Read 03 01 02 01

	Read 03 01 03 01

	Read 03 01 04 01

	Read 03 01 05 01

	Read 03 01 06 01

	Read 03 01 07 01

	Read 03 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 03 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 03)
Seek: 6 -> 6 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 03 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 03 01 09 01 10 0e ff)
	Read 03 01 09 01

	Read 03 01 0a 01

	Read 03 01 0b 01

	Read 03 01 0c 01

	Read 03 01 0d 01

	Read 03 01 0e 01

	Read 03 01 0f 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 03 01 10 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 6 -> 4 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 20)
Seek: 4 -> 64 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 20 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 20 00 09 01 10 0e ff)
	Read 20 00 09 01

	Read 20 00 0a 01

	Read 20 00 0b 01

	Read 20 00 0c 01

	Read 20 00 0d 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 20 00 0e 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 64 -> 4 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 02 01 01 01 10 0e ff)
	Read 02 01 01 01

	Read 02 01 02 01

	Read 02 01 03 01

	Read 02 01 04 01

	Read 02 01 05 01

	Read 02 01 06 01

	Read 02 01 07 01

	Read 02 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 02 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 02 01 09 01 10 0e ff)
	Read 02 01 09 01

	Read 02 01 0a 01

	Read 02 01 0b 01

	Read 02 01 0c 01

	Read 02 01 0d 01

	Read 02 01 0e 01

	Read 02 01 0f 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 02 01 10 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 21)
Seek: 4 -> 66 (62)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 21 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 21 00 01 01 10 0e ff)
	Read 21 00 01 01

	Read 21 00 02 01

	Read 21 00 03 01

	Read 21 00 04 01

	Read 21 00 05 01

	Read 21 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 21 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 66 -> 4 (62)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 09 01 10 0e ff)
	Read 0f 01 09 01

	Read 0f 01 0a 01

	Read 0f 01 0b 01

	Read 0f 01 0c 01

	Read 0f 01 0d 01

	Read 0f 01 0e 01

	Read 0f 01 0f 01

	Read 0f 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 10 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 30 -> 32 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 10 00 01 01 10 0e ff)
	Read 10 00 01 01

	Read 10 00 02 01

	Read 10 00 03 01

	Read 10 00 04 01

	Read 10 00 05 01

	Read 10 00 06 01

	Read 10 00 07 01

	Read 10 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 10 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 32 -> 32 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 10 00 09 01 10 0e ff)
	Read 10 00 09 01

	Read 10 00 0a 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 10 00 0b 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 32 -> 4 (28)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 20)
Seek: 4 -> 64 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 20 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 20 00 09 01 10 0e ff)
	Read 20 00 09 01

	Read 20 00 0a 01

	Read 20 00 0b 01

	Read 20 00 0c 01

	Read 20 00 0d 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 20 00 0e 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 64 -> 4 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 02 01 01 01 10 0e ff)
	Read 02 01 01 01

	Read 02 01 02 01

	Read 02 01 03 01

	Read 02 01 04 01

	Read 02 01 05 01

	Read 02 01 06 01

	Read 02 01 07 01

	Read 02 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 02 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 02 01 09 01 10 0e ff)
	Read 02 01 09 01

	Read 02 01 0a 01

	Read 02 01 0b 01

	Read 02 01 0c 01

	Read 02 01 0d 01

	Read 02 01 0e 01

	Read 02 01 0f 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 02 01 10 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 08 01 10 0e ff)
	Read 02 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 4 -> 74 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 01 01 10 0e ff)
	Read 25 01 01 01

	Read 25 01 02 01

	Read 25 01 03 01

	Read 25 01 04 01

	Read 25 01 05 01

	Read 25 01 06 01

	Read 25 01 07 01

	Read 25 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 25 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 74 -> 74 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 09 01 10 0e ff)
	Read 25 01 09 01

	Read 25 01 0a 01

	Read 25 01 0b 01

	Read 25 01 0c 01

	Read 25 01 0d 01

	Read 25 01 0e 01

	Read 25 01 0f 01

	Read 25 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 26 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 26)
Seek: 74 -> 76 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 26 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 26 00 01 01 10 0e ff)
	Read 26 00 01 01

	Read 26 00 02 01

	Read 26 00 03 01

	Read 26 00 04 01

	Read 26 00 05 01

	Read 26 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 26 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 76 -> 4 (72)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 1a)
Seek: 4 -> 52 (48)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 1a }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 1a 00 01 01 10 0e ff)
	Read 1a 00 01 01

	Read 1a 00 02 01

	Read 1a 00 03 01

	Read 1a 00 04 01

	Read 1a 00 05 01

	Read 1a 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 1a 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 52 -> 4 (48)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 1b)
Seek: 4 -> 54 (50)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 1b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 1b 00 09 01 10 0e ff)
	Read 1b 00 09 01

	Read 1b 00 0a 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 1b 00 0b 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 54 -> 4 (50)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 08 01 10 0e ff)
	Read 02 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 26)
Seek: 4 -> 76 (72)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 26 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 26 00 09 01 10 0e ff)
	Read 26 00 09 01

	Read 26 00 0a 01

	Read 26 00 0b 01

	Read 26 00 0c 01

	Read 26 00 0d 01

	Read 26 00 0e 01

	Read 26 00 0f 01

	Read 26 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 27 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 26)
Seek: 76 -> 76 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 26 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 26 01 01 01 10 0e ff)
	Read 26 01 01 01

	Read 26 01 02 01

	Read 26 01 03 01

	Read 26 01 04 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 26 01 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 76 -> 4 (72)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 4 -> 24 (20)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0c 01 09 01 10 0e ff)
	Read 0c 01 09 01

	Read 0c 01 0a 01

	Read 0c 01 0b 01

	Read 0c 01 0c 01

	Read 0c 01 0d 01

	Read 0c 01 0e 01

	Read 0c 01 0f 01

	Read 0c 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0d 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0d)
Seek: 24 -> 26 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0d }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 0d 00 01 01 10 0e ff)
	Read 0d 00 01 01

	Read 0d 00 02 01

	Read 0d 00 03 01

	Read 0d 00 04 01

	Read 0d 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0d 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 26 -> 4 (22)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 14)
Seek: 4 -> 40 (36)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 14 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 14 00 09 01 10 0e ff)
	Read 14 00 09 01

	Read 14 00 0a 01

	Read 14 00 0b 01

	Read 14 00 0c 01

	Read 14 00 0d 01

	Read 14 00 0e 01

	Read 14 00 0f 01

	Read 14 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 15 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 14)
Seek: 40 -> 40 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 14 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 14 01 01 01 10 0e ff)
	Read 14 01 01 01

	Read 14 01 02 01

	Read 14 01 03 01

	Read 14 01 04 01

	Read 14 01 05 01

	Read 14 01 06 01

	Read 14 01 07 01

	Read 14 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 14 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 14)
Seek: 40 -> 40 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 14 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 14 01 09 01 10 0e ff)
	Read 14 01 09 01

	Read 14 01 0a 01

	Read 14 01 0b 01

	Read 14 01 0c 01

	Read 14 01 0d 01

	Read 14 01 0e 01

	Read 14 01 0f 01

	Read 14 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 15 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 15)
Seek: 40 -> 42 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 15 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 15 00 01 01 10 0e ff)
	Read 15 00 01 01

	Read 15 00 02 01

	Read 15 00 03 01

	Read 15 00 04 01

	Read 15 00 05 01

	Read 15 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 15 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 42 -> 4 (38)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 19)
Seek: 4 -> 50 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 19 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 19 01 01 01 10 0e ff)
	Read 19 01 01 01

	Read 19 01 02 01

	Read 19 01 03 01

	Read 19 01 04 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 19 01 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 50 -> 4 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 20)
Seek: 4 -> 64 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 20 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 20 01 01 01 10 0e ff)
	Read 20 01 01 01

	Read 20 01 02 01

	Read 20 01 03 01

	Read 20 01 04 01

	Read 20 01 05 01

	Read 20 01 06 01

	Read 20 01 07 01

	Read 20 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 20 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 64 -> 4 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 11)
Seek: 4 -> 34 (30)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 11 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 11 00 01 01 10 0e ff)
	Read 11 00 01 01

	Read 11 00 02 01

	Read 11 00 03 01

	Read 11 00 04 01

	Read 11 00 05 01

	Read 11 00 06 01

	Read 11 00 07 01

	Read 11 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 11 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 11)
Seek: 34 -> 34 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 11 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 11 00 09 01 10 0e ff)
	Read 11 00 09 01

	Read 11 00 0a 01

	Read 11 00 0b 01

	Read 11 00 0c 01

	Read 11 00 0d 01

	Read 11 00 0e 01

	Read 11 00 0f 01

	Read 11 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 12 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 11)
Seek: 34 -> 34 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 11 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 11 01 01 01 10 0e ff)
	Read 11 01 01 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 11 01 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 34 -> 4 (30)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 4 -> 22 (18)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0b 00 09 01 10 0e ff)
	Read 0b 00 09 01

	Read 0b 00 0a 01

	Read 0b 00 0b 01

	Read 0b 00 0c 01

	Read 0b 00 0d 01

	Read 0b 00 0e 01

	Read 0b 00 0f 01

	Read 0b 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 01 01 10 0e ff)
	Read 0b 01 01 01

	Read 0b 01 02 01

	Read 0b 01 03 01

	Read 0b 01 04 01

	Read 0b 01 05 01

	Read 0b 01 06 01

	Read 0b 01 07 01

	Read 0b 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0b 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 09 01 10 0e ff)
	Read 0b 01 09 01

	Read 0b 01 0a 01

	Read 0b 01 0b 01

	Read 0b 01 0c 01

	Read 0b 01 0d 01

	Read 0b 01 0e 01

	Read 0b 01 0f 01

	Read 0b 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 22 -> 24 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 01 01 10 0e ff)
	Read 0c 00 01 01

	Read 0c 00 02 01

	Read 0c 00 03 01

	Read 0c 00 04 01

	Read 0c 00 05 01

	Read 0c 00 06 01

	Read 0c 00 07 01

	Read 0c 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 09 01 10 0e ff)
	Read 0c 00 09 01

	Read 0c 00 0a 01

	Read 0c 00 0b 01

	Read 0c 00 0c 01

	Read 0c 00 0d 01

	Read 0c 00 0e 01

	Read 0c 00 0f 01

	Read 0c 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0d 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0c 01 01 01 10 0e ff)
	Read 0c 01 01 01

	Read 0c 01 02 01

	Read 0c 01 03 01

	Read 0c 01 04 01

	Read 0c 01 05 01

	Read 0c 01 06 01

	Read 0c 01 07 01

	Read 0c 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 24 -> 4 (20)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 08 01 10 0e ff)
	Read 02 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 26)
Seek: 4 -> 76 (72)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 26 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 26 00 09 01 10 0e ff)
	Read 26 00 09 01

	Read 26 00 0a 01

	Read 26 00 0b 01

	Read 26 00 0c 01

	Read 26 00 0d 01

	Read 26 00 0e 01

	Read 26 00 0f 01

	Read 26 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 27 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 26)
Seek: 76 -> 76 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 26 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 26 01 01 01 10 0e ff)
	Read 26 01 01 01

	Read 26 01 02 01

	Read 26 01 03 01

	Read 26 01 04 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 26 01 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 76 -> 4 (72)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 4 -> 24 (20)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0c 01 09 01 10 0e ff)
	Read 0c 01 09 01

	Read 0c 01 0a 01

	Read 0c 01 0b 01

	Read 0c 01 0c 01

	Read 0c 01 0d 01

	Read 0c 01 0e 01

	Read 0c 01 0f 01

	Read 0c 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0d 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0d)
Seek: 24 -> 26 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0d }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 0d 00 01 01 10 0e ff)
	Read 0d 00 01 01

	Read 0d 00 02 01

	Read 0d 00 03 01

	Read 0d 00 04 01

	Read 0d 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0d 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 26 -> 4 (22)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 20)
Seek: 4 -> 64 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 20 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 20 01 01 01 10 0e ff)
	Read 20 01 01 01

	Read 20 01 02 01

	Read 20 01 03 01

	Read 20 01 04 01

	Read 20 01 05 01

	Read 20 01 06 01

	Read 20 01 07 01

	Read 20 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 20 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 64 -> 4 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 11)
Seek: 4 -> 34 (30)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 11 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 11 00 01 01 10 0e ff)
	Read 11 00 01 01

	Read 11 00 02 01

	Read 11 00 03 01

	Read 11 00 04 01

	Read 11 00 05 01

	Read 11 00 06 01

	Read 11 00 07 01

	Read 11 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 11 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 11)
Seek: 34 -> 34 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 11 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 11 00 09 01 10 0e ff)
	Read 11 00 09 01

	Read 11 00 0a 01

	Read 11 00 0b 01

	Read 11 00 0c 01

	Read 11 00 0d 01

	Read 11 00 0e 01

	Read 11 00 0f 01

	Read 11 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 12 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 11)
Seek: 34 -> 34 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 11 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 11 01 01 01 10 0e ff)
	Read 11 01 01 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 11 01 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 34 -> 4 (30)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 09)
Seek: 4 -> 18 (14)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 09 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 09 01 01 01 10 0e ff)
	Read 09 01 01 01

	Read 09 01 02 01

	Read 09 01 03 01

	Read 09 01 04 01

	Read 09 01 05 01

	Read 09 01 06 01

	Read 09 01 07 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 09 01 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 18 -> 4 (14)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 1f)
Seek: 4 -> 62 (58)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 1f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 1f 01 01 01 10 0e ff)
	Read 1f 01 01 01

	Read 1f 01 02 01

	Read 1f 01 03 01

	Read 1f 01 04 01

	Read 1f 01 05 01

	Read 1f 01 06 01

	Read 1f 01 07 01

	Read 1f 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 1f 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 1f)
Seek: 62 -> 62 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 1f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 1f 01 09 01 10 0e ff)
	Read 1f 01 09 01

	Read 1f 01 0a 01

	Read 1f 01 0b 01

	Read 1f 01 0c 01

	Read 1f 01 0d 01

	Read 1f 01 0e 01

	Read 1f 01 0f 01

	Read 1f 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 20 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 20)
Seek: 62 -> 64 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 20 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 20 00 01 01 10 0e ff)
	Read 20 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 20 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 64 -> 4 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 20)
Seek: 4 -> 64 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 20 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 20 01 01 01 10 0e ff)
	Read 20 01 01 01

	Read 20 01 02 01

	Read 20 01 03 01

	Read 20 01 04 01

	Read 20 01 05 01

	Read 20 01 06 01

	Read 20 01 07 01

	Read 20 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 20 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 64 -> 4 (60)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 11)
Seek: 4 -> 34 (30)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 11 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 11 00 01 01 10 0e ff)
	Read 11 00 01 01

	Read 11 00 02 01

	Read 11 00 03 01

	Read 11 00 04 01

	Read 11 00 05 01

	Read 11 00 06 01

	Read 11 00 07 01

	Read 11 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 11 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 11)
Seek: 34 -> 34 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 11 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 11 00 09 01 10 0e ff)
	Read 11 00 09 01

	Read 11 00 0a 01

	Read 11 00 0b 01

	Read 11 00 0c 01

	Read 11 00 0d 01

	Read 11 00 0e 01

	Read 11 00 0f 01

	Read 11 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 12 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 11)
Seek: 34 -> 34 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 11 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 11 01 01 01 10 0e ff)
	Read 11 01 01 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 11 01 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 34 -> 4 (30)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 08 01 10 0e ff)
	Read 02 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 4 -> 74 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 25 00 09 01 10 0e ff)
	Read 25 00 09 01

	Read 25 00 0a 01

	Read 25 00 0b 01

	Read 25 00 0c 01

	Read 25 00 0d 01

	Read 25 00 0e 01

	Read 25 00 0f 01

	Read 25 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 26 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 74 -> 4 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 04)
Seek: 4 -> 8 (4)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 04 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 04 01 01 01 10 0e ff)
	Read 04 01 01 01

	Read 04 01 02 01

	Read 04 01 03 01

	Read 04 01 04 01

	Read 04 01 05 01

	Read 04 01 06 01

	Read 04 01 07 01

	Read 04 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 04 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 04)
Seek: 8 -> 8 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 04 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 04 01 09 01 10 0e ff)
	Read 04 01 09 01

	Read 04 01 0a 01

	Read 04 01 0b 01

	Read 04 01 0c 01

	Read 04 01 0d 01

	Read 04 01 0e 01

	Read 04 01 0f 01

	Read 04 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 05 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 05)
Seek: 8 -> 10 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 05 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 05 00 01 01 10 0e ff)
	Read 05 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 05 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 10 -> 4 (6)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 21)
Seek: 4 -> 66 (62)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 21 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 21 00 09 01 10 0e ff)
	Read 21 00 09 01

	Read 21 00 0a 01

	Read 21 00 0b 01

	Read 21 00 0c 01

	Read 21 00 0d 01

	Read 21 00 0e 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 21 00 0f 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 66 -> 4 (62)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 04)
Seek: 4 -> 8 (4)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 04 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 04 00 01 01 10 0e ff)
	Read 04 00 01 01

	Read 04 00 02 01

	Read 04 00 03 01

	Read 04 00 04 01

	Read 04 00 05 01

	Read 04 00 06 01

	Read 04 00 07 01

	Read 04 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 04 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 04)
Seek: 8 -> 8 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 04 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 04 00 09 01 10 0e ff)
	Read 04 00 09 01

	Read 04 00 0a 01

	Read 04 00 0b 01

	Read 04 00 0c 01

	Read 04 00 0d 01

	Read 04 00 0e 01

	Read 04 00 0f 01

	Read 04 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 05 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 8 -> 4 (4)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 08 01 10 0e ff)
	Read 02 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 4 -> 74 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 25 00 09 01 10 0e ff)
	Read 25 00 09 01

	Read 25 00 0a 01

	Read 25 00 0b 01

	Read 25 00 0c 01

	Read 25 00 0d 01

	Read 25 00 0e 01

	Read 25 00 0f 01

	Read 25 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 26 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 74 -> 4 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 04)
Seek: 4 -> 8 (4)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 04 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 04 01 01 01 10 0e ff)
	Read 04 01 01 01

	Read 04 01 02 01

	Read 04 01 03 01

	Read 04 01 04 01

	Read 04 01 05 01

	Read 04 01 06 01

	Read 04 01 07 01

	Read 04 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 04 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 04)
Seek: 8 -> 8 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 04 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 04 01 09 01 10 0e ff)
	Read 04 01 09 01

	Read 04 01 0a 01

	Read 04 01 0b 01

	Read 04 01 0c 01

	Read 04 01 0d 01

	Read 04 01 0e 01

	Read 04 01 0f 01

	Read 04 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 05 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 05)
Seek: 8 -> 10 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 05 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 05 00 01 01 10 0e ff)
	Read 05 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 05 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 10 -> 4 (6)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 11)
Seek: 4 -> 34 (30)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 11 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 11 01 09 01 10 0e ff)
	Read 11 01 09 01

	Read 11 01 0a 01

	Read 11 01 0b 01

	Read 11 01 0c 01

	Read 11 01 0d 01

	Read 11 01 0e 01

	Read 11 01 0f 01

	Read 11 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 12 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 34 -> 4 (30)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 05)
Seek: 4 -> 10 (6)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 05 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 05 00 09 01 10 0e ff)
	Read 05 00 09 01

	Read 05 00 0a 01

	Read 05 00 0b 01

	Read 05 00 0c 01

	Read 05 00 0d 01

	Read 05 00 0e 01

	Read 05 00 0f 01

	Read 05 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 06 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 05)
Seek: 10 -> 10 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 05 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 05 01 01 01 10 0e ff)
	Read 05 01 01 01

	Read 05 01 02 01

	Read 05 01 03 01

	Read 05 01 04 01

	Read 05 01 05 01

	Read 05 01 06 01

	Read 05 01 07 01

	Read 05 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 05 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 05)
Seek: 10 -> 10 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 05 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 05 01 09 01 10 0e ff)
	Read 05 01 09 01

	Read 05 01 0a 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 05 01 0b 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 10 -> 4 (6)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 4 -> 36 (32)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 12 00 01 01 10 0e ff)
	Read 12 00 01 01

	Read 12 00 02 01

	Read 12 00 03 01

	Read 12 00 04 01

	Read 12 00 05 01

	Read 12 00 06 01

	Read 12 00 07 01

	Read 12 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 12 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 36 -> 36 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 12 00 09 01 10 0e ff)
	Read 12 00 09 01

	Read 12 00 0a 01

	Read 12 00 0b 01

	Read 12 00 0c 01

	Read 12 00 0d 01

	Read 12 00 0e 01

	Read 12 00 0f 01

	Read 12 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 13 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 36 -> 36 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 12 01 01 01 10 0e ff)
	Read 12 01 01 01

	Read 12 01 02 01

	Read 12 01 03 01

	Read 12 01 04 01

	Read 12 01 05 01

	Read 12 01 06 01

	Read 12 01 07 01

	Read 12 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 12 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 12)
Seek: 36 -> 36 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 12 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 12 01 09 01 10 0e ff)
	Read 12 01 09 01

	Read 12 01 0a 01

	Read 12 01 0b 01

	Read 12 01 0c 01

	Read 12 01 0d 01

	Read 12 01 0e 01

	Read 12 01 0f 01

	Read 12 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 13 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 36 -> 38 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 13 00 01 01 10 0e ff)
	Read 13 00 01 01

	Read 13 00 02 01

	Read 13 00 03 01

	Read 13 00 04 01

	Read 13 00 05 01

	Read 13 00 06 01

	Read 13 00 07 01

	Read 13 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 13 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 38 -> 38 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 13 00 09 01 10 0e ff)
	Read 13 00 09 01

	Read 13 00 0a 01

	Read 13 00 0b 01

	Read 13 00 0c 01

	Read 13 00 0d 01

	Read 13 00 0e 01

	Read 13 00 0f 01

	Read 13 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 14 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 38 -> 38 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 13 01 01 01 10 0e ff)
	Read 13 01 01 01

	Read 13 01 02 01

	Read 13 01 03 01

	Read 13 01 04 01

	Read 13 01 05 01

	Read 13 01 06 01

	Read 13 01 07 01

	Read 13 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 13 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 13)
Seek: 38 -> 38 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 13 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 13 01 09 01 10 0e ff)
	Read 13 01 09 01

	Read 13 01 0a 01

	Read 13 01 0b 01

	Read 13 01 0c 01

	Read 13 01 0d 01

	Read 13 01 0e 01

	Read 13 01 0f 01

	Read 13 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 14 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 14)
Seek: 38 -> 40 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 14 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 14 00 01 01 10 0e ff)
	Read 14 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 14 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 40 -> 4 (36)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 08 01 10 0e ff)
	Read 02 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 4 -> 74 (70)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 01 01 10 0e ff)
	Read 25 01 01 01

	Read 25 01 02 01

	Read 25 01 03 01

	Read 25 01 04 01

	Read 25 01 05 01

	Read 25 01 06 01

	Read 25 01 07 01

	Read 25 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 25 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 25)
Seek: 74 -> 74 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 25 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 25 01 09 01 10 0e ff)
	Read 25 01 09 01

	Read 25 01 0a 01

	Read 25 01 0b 01

	Read 25 01 0c 01

	Read 25 01 0d 01

	Read 25 01 0e 01

	Read 25 01 0f 01

	Read 25 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 26 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 26)
Seek: 74 -> 76 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 26 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 26 00 01 01 10 0e ff)
	Read 26 00 01 01

	Read 26 00 02 01

	Read 26 00 03 01

	Read 26 00 04 01

	Read 26 00 05 01

	Read 26 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 26 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 76 -> 4 (72)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0e)
Seek: 4 -> 28 (24)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0e }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0e 01 09 01 10 0e ff)
	Read 0e 01 09 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0e 01 0a 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 28 -> 4 (24)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 19)
Seek: 4 -> 50 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 19 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 19 01 01 01 10 0e ff)
	Read 19 01 01 01

	Read 19 01 02 01

	Read 19 01 03 01

	Read 19 01 04 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 19 01 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 50 -> 4 (46)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 24)
Seek: 4 -> 72 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 24 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 24 01 01 01 10 0e ff)
	Read 24 01 01 01

	Read 24 01 02 01

	Read 24 01 03 01

	Read 24 01 04 01

	Read 24 01 05 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 24 01 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 72 -> 4 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 4 -> 32 (28)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 10 01 01 01 10 0e ff)
	Read 10 01 01 01

	Read 10 01 02 01

	Read 10 01 03 01

	Read 10 01 04 01

	Read 10 01 05 01

	Read 10 01 06 01

	Read 10 01 07 01

	Read 10 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 10 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 10)
Seek: 32 -> 32 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 10 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 10 01 09 01 10 0e ff)
	Read 10 01 09 01

	Read 10 01 0a 01

	Read 10 01 0b 01

	Read 10 01 0c 01

	Read 10 01 0d 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 10 01 0e 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 32 -> 4 (28)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0f)
Seek: 4 -> 30 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0f }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0f 01 01 01 10 0e ff)
	Read 0f 01 01 01

	Read 0f 01 02 01

	Read 0f 01 03 01

	Read 0f 01 04 01

	Read 0f 01 05 01

	Read 0f 01 06 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0f 01 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 30 -> 4 (26)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 4 -> 22 (18)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0b 00 09 01 10 0e ff)
	Read 0b 00 09 01

	Read 0b 00 0a 01

	Read 0b 00 0b 01

	Read 0b 00 0c 01

	Read 0b 00 0d 01

	Read 0b 00 0e 01

	Read 0b 00 0f 01

	Read 0b 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 01 01 10 0e ff)
	Read 0b 01 01 01

	Read 0b 01 02 01

	Read 0b 01 03 01

	Read 0b 01 04 01

	Read 0b 01 05 01

	Read 0b 01 06 01

	Read 0b 01 07 01

	Read 0b 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0b 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0b)
Seek: 22 -> 22 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0b }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(04 0b 01 09 01 10 0e ff)
	Read 0b 01 09 01

	Read 0b 01 0a 01

	Read 0b 01 0b 01

	Read 0b 01 0c 01

	Read 0b 01 0d 01

	Read 0b 01 0e 01

	Read 0b 01 0f 01

	Read 0b 01 10 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 22 -> 24 (2)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 01 01 10 0e ff)
	Read 0c 00 01 01

	Read 0c 00 02 01

	Read 0c 00 03 01

	Read 0c 00 04 01

	Read 0c 00 05 01

	Read 0c 00 06 01

	Read 0c 00 07 01

	Read 0c 00 08 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0c 00 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 0c 00 09 01 10 0e ff)
	Read 0c 00 09 01

	Read 0c 00 0a 01

	Read 0c 00 0b 01

	Read 0c 00 0c 01

	Read 0c 00 0d 01

	Read 0c 00 0e 01

	Read 0c 00 0f 01

	Read 0c 00 10 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 0d 00 01 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 0c)
Seek: 24 -> 24 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 0c }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(04 0c 01 01 01 10 0e ff)
	Read 0c 01 01 01

	Read 0c 01 02 01

	Read 0c 01 03 01

	Read 0c 01 04 01

	Read 0c 01 05 01

	Read 0c 01 06 01

	Read 0c 01 07 01

	Read 0c 01 08 01

 <TC>	TC at 0x100 byte
	{ 04 00 00 0c 01 09 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 24 -> 4 (20)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 2c }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 01 01 10 0e ff)
	Read 02 00 01 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 02 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 02 01 10 0e ff)
	Read 02 00 02 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 03 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 03 01 10 0e ff)
	Read 02 00 03 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 04 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 04 01 10 0e ff)
	Read 02 00 04 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 05 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 05 01 10 0e ff)
	Read 02 00 05 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 06 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 06 01 10 0e ff)
	Read 02 00 06 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 07 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 02)
Seek: 4 -> 4 (0)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 02 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 02 00 07 01 10 0e ff)
	Read 02 00 07 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 02 00 08 01 }
FD 0 Off

[0f] Seek FD 0 On
(00 24)
Seek: 4 -> 72 (68)
FD 0 Off
	Seek (0) success.

[08] SenceIntStatus 	{ 20 24 }
FD 0 Off

[04] SenceDeviceStatus FD 0 On
(00) 	{ 28 }
FD 0 Off

[46] ReadData FD 0 On
(00 24 00 09 01 10 0e ff)
	Read 24 00 09 01

	Read 24 00 0a 01

 <TC>	TC at 0x100 byte
	{ 00 00 00 24 00 0b 01 }
FD 0 Off
